****************************************************************

  lasview:

  A simple OpenGL-based viewer for LIDAR in LAS/LAZ/ASCII format
  that can also edit or delete points as well as compute/display
  a TIN computed from (a selection of) the points.

  EDITING & DELETING POINTS

  Press <e> to start r<e>classifying point as noise (7). Use the
  pop-up menu (right click) to select other target classes. Draw
  a polygon enclosing some points and press <r> to register the
  operation. With <ESC> you can unset the last polygon point and
  with <CTRL+u> you can undo the operation or with <CTRL+o> redo
  it again.

  Press <d> to start <d>eleting points. Otherwise same procedure
  as above.

  When finished press <CTRL+s> to save the edits as LASlayers in
  to a LAY file. Warning ... if you did not start lasview with
  the '-ilay' option you will not append to an existing LAY file
  but overwrite it. There will be a WARNING though. Later, you
  can check your layers of edits with 'laslayers.exe' or view
  and continue editing with the '-ilay' option when starting
  lasview again.

  If you want to apply your edits and creating a new file press
  <CTRL-a> and an entirely new file (currently with "_1" at the
  end of the input file name) is created.

  Do not use lasview with on-the-fly filters or transforms when
  you plan to do editing operations that you are going to save.

  VIEWING AND TRAVERSING CROSS SECTIONS 

  For quality checking and detail views you can press <x> and
  select a cross section or smaller area of interest. Move it
  around with the arrow key. Holding down <SHIFT> or <ALT> is
  taking larger or smaller steps. Press <x> again and you see
  only the selected area. Again, traverse the LiDAR my moving
  around with the arrow keys. You can do your edits in this
  cross section view. Jumping back between cross section view
  and the full extend with <x> help maintaining orientation.

  With <CTRL-x> you can end the cross section view.

  Please contact martin.isenburg@rapidlasso.com if you want to
  use lasview commercially.

  For updates check the website or join the LAStools mailing list.

  http://lastools.org/
  http://groups.google.com/group/lastools/
  http://twitter.com/lastools/
  http://facebook.com/lastools/
  http://linkedin.com/groups?gid=4408378

  Martin @rapidlasso

****************************************************************

example usage:

>> lasview lidar.las
>> lasview -i lidar.las

reads around 1000000 subsampled lidar points and displays in 50 steps

>> lasview *.las

merges all LAS files into one and displays a subsampling of it

>> lasview -i lidar.txt -iparse xyzc

converts an ASCII file on-the-fly with parse string 'xyzc' and displays it

>> lasview -i lidar.las -win 1600 1200

same as above but with a larger display window

>> lasview -i lidar.las -steps 10 -points 10000000

reads around 10 million subsampled lidar points and displays in 11 steps

interactive options:

<t>     compute a TIN from the displayed returns
<T>     remove the TIN
<h>     change shading mode for TIN (hill-shade, elevation, wire-frame)

<a>     display all returns
<l>     display last returns only
<f>     display first returns only
<g>     display returns classified as ground
<b>     display returns classified as building
<B>     display returns classified as building + ground
<v>     display returns classified as vegetation
<V>     display returns classified as vegetation + ground
<j>     display returns classified as building + vegetation
<J>     display returns classified as building + vegetation + ground
<m>     display returns classified as keypoints / mass points
<n>     display returns classified as noise
<o>     display returns classified as overlap
<w>     display returns classified as water
<u>     display returns that are unclassified
<0>     display ((point source IDs % 8) == 0)
<1>     display ((point source IDs % 8) == 1)
<2>     display ((point source IDs % 8) == 2)
<3>     display ((point source IDs % 8) == 3)
<4>     display ((point source IDs % 8) == 4)
<5>     display ((point source IDs % 8) == 5)
<6>     display ((point source IDs % 8) == 6)
<7>     display ((point source IDs % 8) == 7)

<e>      start editing points
<d>      start deleting points
<r>      register edit / delete operation

<CTRL-u> undo last changes
<CTRL-o> redo last undo

<CTRL-s> save changes as LASlayers
<CTRL-f> force LAY file overwrite
<CTRL-a> apply LASlayers to create new LAS/LAZ file

<i>      pick a point
<x>      toggle between cross-section and overview
<CTRL-x> turn cross-section view on / off

<SHIFT> translate mode
<CTRL>  zoom mode
<ALT>   pan mode
<space> switch between pan/translate/zoom/tilt
<-/=>   render points smaller/bigger
<[/]>   scale elevation
<{/}>   scale xy plane
<c>     change color mode
<X>     hide/show bounding box
<s/S>   step forward/backward
<z/Z>   tiny step forward/backward

<A>     toggle adaptive Z-scaling on/off
<Q>     show spatial index structure (if LAX file available)
<q>     pick spatial index cell
<W>     show LAS 1.3 waveforms +/- 25 points around picked point

C:\lastools\bin>lasview.exe -h
Filter points based on their coordinates.
  -keep_tile 631000 4834000 1000 (ll_x ll_y size)
  -keep_circle 630250.00 4834750.00 100 (x y radius)
  -keep_xy 630000 4834000 631000 4836000 (min_x min_y max_x max_y)
  -drop_xy 630000 4834000 631000 4836000 (min_x min_y max_x max_y)
  -keep_x 631500.50 631501.00 (min_x max_x)
  -drop_x 631500.50 631501.00 (min_x max_x)
  -drop_x_below 630000.50 (min_x)
  -drop_x_above 630500.50 (max_x)
  -keep_y 4834500.25 4834550.25 (min_y max_y)
  -drop_y 4834500.25 4834550.25 (min_y max_y)
  -drop_y_below 4834500.25 (min_y)
  -drop_y_above 4836000.75 (max_y)
  -keep_z 11.125 130.725 (min_z max_z)
  -drop_z 11.125 130.725 (min_z max_z)
  -drop_z_below 11.125 (min_z)
  -drop_z_above 130.725 (max_z)
  -keep_xyz 620000 4830000 100 621000 4831000 200 (min_x min_y min_z max_x max_y max_z)
  -drop_xyz 620000 4830000 100 621000 4831000 200 (min_x min_y min_z max_x max_y max_z)
Filter points based on their return number.
  -first_only -keep_first -drop_first
  -last_only -keep_last -drop_last
  -keep_middle -drop_middle
  -keep_return 1 2 3
  -drop_return 3 4
  -keep_single -drop_single
  -keep_double -drop_double
  -keep_triple -drop_triple
  -keep_quadruple -drop_quadruple
  -keep_quintuple -drop_quintuple
Filter points based on the scanline flags.
  -drop_scan_direction 0
  -scan_direction_change_only
  -edge_of_flight_line_only
Filter points based on their intensity.
  -keep_intensity 20 380
  -drop_intensity_below 20
  -drop_intensity_above 380
  -drop_intensity_between 4000 5000
Filter points based on their classification.
  -keep_class 1 3 7
  -drop_class 4 2
  -drop_synthetic -keep_synthetic
  -drop_keypoint -keep_keypoint
  -drop_withheld -keep_withheld
Filter points based on their user data.
  -keep_user_data 1
  -drop_user_data 255
  -keep_user_data_between 10 20
  -drop_user_data_below 1
  -drop_user_data_above 100
  -drop_user_data_between 10 40
Filter points based on their point source ID.
  -keep_point_source 3
  -keep_point_source_between 2 6
  -drop_point_source 27
  -drop_point_source_below 6
  -drop_point_source_above 15
  -drop_point_source_between 17 21
Filter points based on their scan angle.
  -keep_scan_angle -15 15
  -drop_abs_scan_angle_above 15
  -drop_scan_angle_below -15
  -drop_scan_angle_above 15
  -drop_scan_angle_between -25 -23
Filter points based on their gps time.
  -keep_gps_time 11.125 130.725
  -drop_gps_time_below 11.125
  -drop_gps_time_above 130.725
  -drop_gps_time_between 22.0 48.0
Filter points based on their wavepacket.
  -keep_wavepacket 0
  -drop_wavepacket 3
Filter points with simple thinning.
  -keep_every_nth 2
  -keep_random_fraction 0.1
  -thin_with_grid 1.0
Transform coordinates.
  -translate_x -2.5
  -scale_z 0.3048
  -rotate_xy 15.0 620000 4100000 (angle + origin)
  -translate_xyz 0.5 0.5 0
  -translate_then_scale_y -0.5 1.001
  -clamp_z_below 70.5
  -clamp_z 70.5 72.5
Transform raw xyz integers.
  -translate_raw_z 20
  -translate_raw_xyz 1 1 0
  -clamp_raw_z 500 800
Transform intensity.
  -scale_intensity 2.5
  -translate_intensity 50
  -translate_then_scale_intensity 0.5 3.1
  -clamp_intensity 0 255
  -clamp_intensity_above 255
Transform scan_angle.
  -scale_scan_angle 1.944445
  -translate_scan_angle -5
  -translate_then_scale_scan_angle -0.5 2.1
Change the return number or return count of points.
  -repair_zero_returns
  -set_return_number 1
  -change_return_number_from_to 2 1
  -set_number_of_returns 2
  -change_number_of_returns_from_to 0 2
Modify the classification.
  -set_classification 2
  -change_classification_from_to 2 4
  -classify_z_below_as -5.0 7
  -classify_z_above_as 70.0 7
  -classify_z_between_as 2.0 5.0 4
  -classify_intensity_above_as 200 9
  -classify_intensity_below_as 30 11
Modify the user data.
  -set_user_data 0
  -change_user_data_from_to 23 26
Modify the point source ID.
  -set_point_source 500
  -change_point_source_from_to 1023 1024
  -quantize_Z_into_point_source 200
Transform gps_time.
  -translate_gps_time 40.50
  -adjusted_to_week
  -week_to_adjusted 1671
Transform RGB colors.
  -scale_rgb_down (by 256)
  -scale_rgb_up (by 256)
Supported LAS Inputs
  -i lidar.las
  -i lidar.laz
  -i lidar1.las lidar2.las lidar3.las -merged
  -i *.las - merged
  -i flight0??.laz flight1??.laz
  -i terrasolid.bin
  -i esri.shp
  -i nasa.qi
  -i lidar.txt -iparse xyzti -iskip 2 (on-the-fly from ASCII)
  -i lidar.txt -iparse xyzi -itranslate_intensity 1024
  -lof file_list.txt
  -stdin (pipe from stdin)
  -rescale 0.01 0.01 0.001
  -rescale_xy 0.01 0.01
  -rescale_z 0.01
  -reoffset 600000 4000000 0
Supported LAS Outputs
  -o lidar.las
  -o lidar.laz
  -o xyzta.txt -oparse xyzta (on-the-fly to ASCII)
  -o terrasolid.bin
  -o nasa.qi
  -odir C:\data\ground (specify output directory)
  -odix _classified (specify file name appendix)
  -ocut 2 (cut the last two characters from name)
  -olas -olaz -otxt -obin -oqfit (specify format)
  -stdout (pipe to stdout)
  -nil    (pipe to NULL)
LAStools (by martin@rapidlasso.com) version 140301 (unlicensed)
usage:
lasnoise -i in.laz -o out.laz
lasnoise -i raw\*.laz -step 2 -isolated 3 -odir D:\denoised -olaz
lasnoise -i *.laz -step 4 -isolated 5 -olaz -remove_noise
lasnoise -i *.laz -step 3 -isolated 10 -olaz -flag_as_withheld
lasnoise -i tiles\*.laz -step 3 -isolated 3 -classify_as 31 -odir denoised -olaz
lasnoise -h

D:\lastools\bin>
D:\lastools\bin>
D:\lastools\bin>
D:\lastools\bin>
D:\lastools\bin>
D:\lastools\bin>
D:\lastools\bin>
D:\lastools\bin>
D:\lastools\bin>
D:\lastools\bin>
D:\lastools\bin>
D:\lastools\bin>
D:\lastools\bin>lasview -h
Filter points based on their coordinates.
  -keep_tile 631000 4834000 1000 (ll_x ll_y size)
  -keep_circle 630250.00 4834750.00 100 (x y radius)
  -keep_xy 630000 4834000 631000 4836000 (min_x min_y max_x max_y)
  -drop_xy 630000 4834000 631000 4836000 (min_x min_y max_x max_y)
  -keep_x 631500.50 631501.00 (min_x max_x)
  -drop_x 631500.50 631501.00 (min_x max_x)
  -drop_x_below 630000.50 (min_x)
  -drop_x_above 630500.50 (max_x)
  -keep_y 4834500.25 4834550.25 (min_y max_y)
  -drop_y 4834500.25 4834550.25 (min_y max_y)
  -drop_y_below 4834500.25 (min_y)
  -drop_y_above 4836000.75 (max_y)
  -keep_z 11.125 130.725 (min_z max_z)
  -drop_z 11.125 130.725 (min_z max_z)
  -drop_z_below 11.125 (min_z)
  -drop_z_above 130.725 (max_z)
  -keep_xyz 620000 4830000 100 621000 4831000 200 (min_x min_y min_z max_x max_y max_z)
  -drop_xyz 620000 4830000 100 621000 4831000 200 (min_x min_y min_z max_x max_y max_z)
Filter points based on their return number.
  -first_only -keep_first -drop_first
  -last_only -keep_last -drop_last
  -keep_middle -drop_middle
  -keep_return 1 2 3
  -drop_return 3 4
  -keep_single -drop_single
  -keep_double -drop_double
  -keep_triple -drop_triple
  -keep_quadruple -drop_quadruple
  -keep_quintuple -drop_quintuple
Filter points based on the scanline flags.
  -drop_scan_direction 0
  -scan_direction_change_only
  -edge_of_flight_line_only
Filter points based on their intensity.
  -keep_intensity 20 380
  -drop_intensity_below 20
  -drop_intensity_above 380
  -drop_intensity_between 4000 5000
Filter points based on their classification.
  -keep_class 1 3 7
  -drop_class 4 2
  -drop_synthetic -keep_synthetic
  -drop_keypoint -keep_keypoint
  -drop_withheld -keep_withheld
Filter points based on their user data.
  -keep_user_data 1
  -drop_user_data 255
  -keep_user_data_between 10 20
  -drop_user_data_below 1
  -drop_user_data_above 100
  -drop_user_data_between 10 40
Filter points based on their point source ID.
  -keep_point_source 3
  -keep_point_source_between 2 6
  -drop_point_source 27
  -drop_point_source_below 6
  -drop_point_source_above 15
  -drop_point_source_between 17 21
Filter points based on their scan angle.
  -keep_scan_angle -15 15
  -drop_abs_scan_angle_above 15
  -drop_scan_angle_below -15
  -drop_scan_angle_above 15
  -drop_scan_angle_between -25 -23
Filter points based on their gps time.
  -keep_gps_time 11.125 130.725
  -drop_gps_time_below 11.125
  -drop_gps_time_above 130.725
  -drop_gps_time_between 22.0 48.0
Filter points based on their wavepacket.
  -keep_wavepacket 0
  -drop_wavepacket 3
Filter points with simple thinning.
  -keep_every_nth 2
  -keep_random_fraction 0.1
  -thin_with_grid 1.0
Transform coordinates.
  -translate_x -2.5
  -scale_z 0.3048
  -rotate_xy 15.0 620000 4100000 (angle + origin)
  -translate_xyz 0.5 0.5 0
  -translate_then_scale_y -0.5 1.001
  -clamp_z_below 70.5
  -clamp_z 70.5 72.5
Transform raw xyz integers.
  -translate_raw_z 20
  -translate_raw_xyz 1 1 0
  -clamp_raw_z 500 800
Transform intensity.
  -scale_intensity 2.5
  -translate_intensity 50
  -translate_then_scale_intensity 0.5 3.1
  -clamp_intensity 0 255
  -clamp_intensity_above 255
Transform scan_angle.
  -scale_scan_angle 1.944445
  -translate_scan_angle -5
  -translate_then_scale_scan_angle -0.5 2.1
Change the return number or return count of points.
  -repair_zero_returns
  -set_return_number 1
  -change_return_number_from_to 2 1
  -set_number_of_returns 2
  -change_number_of_returns_from_to 0 2
Modify the classification.
  -set_classification 2
  -change_classification_from_to 2 4
  -classify_z_below_as -5.0 7
  -classify_z_above_as 70.0 7
  -classify_z_between_as 2.0 5.0 4
  -classify_intensity_above_as 200 9
  -classify_intensity_below_as 30 11
Modify the user data.
  -set_user_data 0
  -change_user_data_from_to 23 26
Modify the point source ID.
  -set_point_source 500
  -change_point_source_from_to 1023 1024
  -quantize_Z_into_point_source 200
Transform gps_time.
  -translate_gps_time 40.50
  -adjusted_to_week
  -week_to_adjusted 1671
Transform RGB colors.
  -scale_rgb_down (by 256)
  -scale_rgb_up (by 256)
Supported LAS Inputs
  -i lidar.las
  -i lidar.laz
  -i lidar1.las lidar2.las lidar3.las -merged
  -i *.las - merged
  -i flight0??.laz flight1??.laz
  -i terrasolid.bin
  -i esri.shp
  -i nasa.qi
  -i lidar.txt -iparse xyzti -iskip 2 (on-the-fly from ASCII)
  -i lidar.txt -iparse xyzi -itranslate_intensity 1024
  -lof file_list.txt
  -stdin (pipe from stdin)
  -rescale 0.01 0.01 0.001
  -rescale_xy 0.01 0.01
  -rescale_z 0.01
  -reoffset 600000 4000000 0
Supported LAS Outputs
  -o lidar.las
  -o lidar.laz
  -o xyzta.txt -oparse xyzta (on-the-fly to ASCII)
  -o terrasolid.bin
  -o nasa.qi
  -odir C:\data\ground (specify output directory)
  -odix _classified (specify file name appendix)
  -ocut 2 (cut the last two characters from name)
  -olas -olaz -otxt -obin -oqfit (specify format)
  -stdout (pipe to stdout)
  -nil    (pipe to NULL)
LAStools (by martin.isenburg@rapidlasso.com) version 140301
usage:
lasview -i terrain.las -v
lasview -i flight1*.laz flight2*.laz
lasview -i lidar1.las lidar2.las lidar3.las
lasview -i *.txt -iparse xyz
lasview -i lidar.laz -win 1600 1200 -steps 10 -points 200000
lasview -i lidar.laz -subseq 10000 20000
lasview -h

----

if you find bugs let me (martin.isenburg@rapidlasso.com) know
